MATERIAL SAFETY DATA SHEET

Section I. Product Identification and Uses

Product Identifier: Fungal Shield Surface Protectant
Product Code: 3510
Class:  NON-HAZ
IHC: 3824.90.91.50
Supplier: EcoChem
Address: 231 2nd. Ave. Hanna, AB, Canada 
Tel: 403-364-2888  /  403-364-2802
Fax: 403-364-2889

HFRP - HMIS:
Health Hazard: 1
Fire Hazard:     0
Reactivity:        0
Personal Prot:  1

Section II. Hazardous Ingredients

Name                            		              CAS #       % by Weight    TLV/PEL                LC50/LD50
Octadecylaminodemethyl ammonium chloride  6834-92-0        1-5        	   Not available.      ORAL (LD50): Acute: 600 mg/kg [Rat.].
Methanol                                                           1310-58-3         1-5            Not available.      ORAL (LD50): Acute: 365 mg/kg [Rat.].
Chloropropyl trimethoxysilane                          26027-38-3        1-5        	   Not available.      ORAL (LD50): Acute: 2590 mg/kg [Rat.].             DERMAL (LD50): Acute: 2830 mg/kg [Rabbit.]. 
		
Section III. Physical Data

Physical state and appearance: 		Liquid. (Clear liquid)
Color: 					Colorless or pale yellow
Odor: 					Characteristic.
pH: 					(Concentrate) 13.4 [Basic.] 
Volatility: 				89% (v/v).
Boiling point: 				NA
Vapor density: 				Weighted average: 1 (Air = 1)
Specific gravity: 			1.030-1.050 (Water = 1)
Vapor pressure: 				The highest known value is 17.2 mm Hg (@ 20°C) (Water).
Solubility: 				Easily soluble in cold water, hot water, methanol. Soluble in diethyl ether.  Slightly soluble in n-octanol.

Section IV. Fire and Explosion Data

The product is: 				Non-flammable.
Auto-ignition temperature: 		Not applicable.
Flash points: 				Not applicable.
Degradation products: 			Carbon oxides (CO, CO2) nitrogen oxides (NO, NO2...)
Extinguishing media:			DRY chemicals, CO2, water spray or foam.

Section V. Reactivity Data

Stability: 				The product is stable.
Decomp. products: 			See fire degradation products.
Reactivity: 				Incompatible with oxidizing agents, acids, reducing agents, organic materials, metals, alkalis.

Section VI. Toxicological Properties

Routes of entry: 				Eye contact, Ingestion, Inhalation, Skin contact.
Toxicity for animals: 			Acute oral toxicity (LD50): 4100 mg/kg (RAT) (Calculated value).

Acute effects: 				In case of skin and eye contact (corrosive) – In case of ingestion (corrosive to digestive system). Liquid or spray mist may produce tissue damage. May be harmful if inhaled.

Chronic effects: 				Carcinogenic effects: Not available. 
					Mutagenic effects: Not available. 
					Teratogenic effects: Not available.
Developmental toxicity: Not available.

Section VIII. First Aid Measures

Eye contact: Flush eyes with running water keeping eyelids open. If irritation persists, seek medical attention.

Skin contact: Gently and thoroughly wash the contaminated skin with running water and non-abrasive soap. If irritation persists, seek medical attention. 

Inhalation: Allow the victim to rest in a well ventilated area. Seek medical attention.

Ingestion: DO NOT induce vomiting. Have conscious person drink several glasses water.

Section VIII. Preventive Measures

Waste disposal: 	Dispose of material according to regional, provincial and federal regulations. 
	              	Consult regulators before disposing of large quantities.

Storage: 	Store in a dry, cool and well ventilated area. 

Precautions: 	Keep container dry. DO NOT ingest. If ingested, seek medical advice immediately and show the container or the label. Avoid contact with skin and eyes. Avoid breathing vapors or spray mists. Do not use in food areas.

Spill and leak: 	Absorb with an inert DRY material and place in an appropriate waste disposal container. Dispose of in accordance with federal, provincial, or local regulations.

Section IX. Personal protective equipment

Gloves: 		Gloves (impervious)

Respiratory:	In case of insufficient ventilation wear suitable respiratory equipment.

Eyes: 		Splash goggles.

Other: 		Under exceptional circumstances such as fire, spill or fprolonged contact with bulk quantities, boots, face shield are recommended.

Eng. controls: 	Use exhaust ventilation or other engineering controls to keep the airborne concentrations of vapors below their respective threshold limit value. Ensure that eyewash stations and safety showers are proximal to the workstation location.

Section X. Compliance

COMPLIANCE
Fully complies with EPA Toxic Substance Control Act (TSCA) and the rules, orders and regulations promulgated there under including:
a) Sections 4, 5, 6 & 7; Title 40 Chapter 1, 707.20 thru 707.75;
b) 40 CFR Sections 704.3. 710.2(e) and 720.3(c); and
c) Sections 5 and 13, reference 42FR64583
d) Does not contain marine pollutants as defined in 49 CFR 171.8.
e) Does not contain fungal organisms, microbial organisms, animal or plant components.

Section XI. Preparation and other Information

Prepared by: MSDS Coordinator, June 20th  2002 - REV. Jan. 4th 2006

To the best of our knowledge, the information contained herein is accurate. However, neither the above named supplier nor any of its subsidiaries assumes any liability whatsoever for the accuracy or completeness of the information contained herein. Final determination of suitability of any material is the sole responsibility of the user. All materials may present unknown hazards and should be used with caution. Although certain hazards are described herein, we cannot guarantee that these are the only hazards that exist.

BACK TO MAIN WINDOW